/* This is a linker parameter file for the MC68HLC908QY4 */

NAMES END /* CodeWarrior will pass all the needed files to the linker by command line. But here you may add your own files too. */

SEGMENTS /* Here all RAM/ROM areas of the device are listed. Used in PLACEMENT below. */
    ROM                      =  READ_ONLY    0xEE00 TO 0xFDFF;
    Z_RAM                    =  READ_WRITE   0x0080 TO 0x00FF;
    ROM1                     =  READ_ONLY    0xFFB0 TO 0xFFBD;
    ROM2                     =  READ_ONLY    0xFFC2 TO 0xFFCF;
END

PLACEMENT /* Here all predefined and user segments are placed into the SEGMENTS defined above. */
    DEFAULT_ROM, ROM_VAR, STRINGS       INTO  ROM; /* ROM1,ROM2 In case you want to use ROM1,ROM2 as well, be sure the option -OnB=b is passed to the compiler. */
    DEFAULT_RAM,
    _DATA_ZEROPAGE, MY_ZEROPAGE         INTO  Z_RAM;
END


STACKSIZE 0x30

VECTOR 0 _Startup /* Reset vector: this is the default entry point for an application. */
