;version 1.09, 06/20/2002, Copyright P&E Microcomputer Systems, www.pemicro.com
;device Motorola, 68HC908QT4, All
;begin_cs 
REQUIRES_PROG_VERSION=1.63/
WRITE_BYTE=01/0000001F/       ;Clear COP Watchdog
WRITE_BYTE=09/0000000B/       ;Enable PORTA pullups
WRITE_BYTE=01/0000001E/	      ;Enable Reset pin 
TRIM_QTQY_FREQ=3200000/       ;Desired trimmed bus frequency
BLANK_MODULE_ONLY
SRECORD_SECTION_MASK=FFFF0FFF/   ;overlapping algorithm routines
NO_BASE_ADDRESS=0000EE00/     ;Fixed at $EE00
ADDR_RANGE=00000000/00000FFF/ ; $EE00-$FDFF
ADDR_RANGE=000011B0/000011FF/ ; $FFB0-$FFFF
BLOCKW_QTQY=000000D2/
SHORT_TABLE  ; Use a table of word addresses
;end_cs
;
S113208C0080008C002CEE001200109E000000005A
S113209C0000108C00B800000000000040A10000FB
S10720AC000000002C
S113408CB7867F6F01E601BB83E701F6B982F73B84
S113409C86F3AF0281A60A42AE0352B7878C5F83C4
S11300B84E8789B6854ABB83B78BB684B982B78A1B
S10B00C85582CD28098C5F83E9
S113108C4E87896E40886EE08A6E008B45E000CDF9
S113109C28066E10864F45EE00AD1645FFBEF6438E
S11310AC261C6E0186A65045FFB0AD053F843F85D6
S11310BC83732608AF014BF93B86F6818686AF0114
S10410CC839C
S9030000FC
~